1. Restart Server and goto BIOS settings

2. Press **F3 Optimized** **defaults** due to GUI based AVAGO MegaRAID configuration Utility to show (Note: AVAGO MegaRAID configuration Utility default save to server)

3. After default settings restart server and goto BIOS settings (Del key Press)

4. Goto **Advanced Configuration** and select PCIe/PCI/PnP. To change settings Legacy to EFI below details due to show AVAGO MegaRAID configuration Utility.

Onboard NVM E1 OPROM EFI

Onboard NVM E2 OPROM EFI

CPU1 Slot1 PCI-E x 8 OPROM EFI

CPU2 Slot1 PCI-E x 16 OPROM EFI

CPU3 Slot1 PCI-E x 8 OPROM EFI

CPU4 Slot1 PCI-E x 16 OPROM EFI

CPU5 Slot1 PCI-E x 16 OPROM EFI

CPU6 Slot1 PCI-E x 16 OPROM EFI

5. Booting Option to select UEFI Hard disk OS and restart.

**6. Management Console activated and Server details sheet updated via BIOS settings**